G100 HD

Upgrade device by USB;

Put upgrade mode on All mode .



How to do Recovery by Usb : (boot)

1-first of all format the Usb.
2-Its file rename to gxrom.bin
3-Plug in the usb to the device then power ON.
 
It will auto upgrade and recovery.



Key of activtion patch ; 8989
Press 8989 on Utility part in main menu.

Master code : 8765



F3 : Antenna Setting
F4 : Motor Setting
00000 : Network
99999 : Server